Driver_Auto_Installer_v1.1208.00

ReadMe.txt

This application will install USB com port driver for MediaTek's device those IDs are listed below:

1."VID_0E8D&PID_0003"       (FeaturePhone & Smartphone BootROM - MTK USB Port)
2."VID_0E8D&PID_0023&MI_00" (FeaturePhone - MTK USB Modem Port)
3."VID_0E8D&PID_0023&MI_02" (FeaturePhone - MTK USB Debug Port)
4."VID_0E8D&PID_2000"       (SmartPhone - Preloaer USB Port)
5."VID_0E8D&PID_2001"       (SmartPhone - DA USB Port)
6."Vid_0E8D&PID_2006&MI_02" (SmartPhone - Kernel Gadget USB port, Please customize your kernel VID/PID)
  "Vid_0E8D&PID_2007"
  "Vid_0E8D&PID_200a&MI_02" 

注意: 实际Meta Mode手机Kernel软件串口VID/PID是"Vid_0BB4&PID_0005&MI_02", 默认请使用Android Tool Package/driver(binary)中Android_Gadget_CDC_driver.inf PC驱动.
      如果需要使用本install tool, 请参考usb客制化文档调整为"Vid_0E8D&PID_2006&MI_02"才能使用本驱动包.


The application user must belong to Administrator group or have the privilege to install driver.

the execution of the InstallDriver.exe will install the driver, and the UninstallDriver.exe is special for remove driver.
the InstallDriver.exe will remove the legacy version of driver before install current driver automatically.

Notes:
1. Windows 2003 use the INF files which under the 2K_XP_COM
2. The device which generates two com ports (USB Modem Port Driver & USB Modem Debug Driver) only support Systems after Win XP sp3 version. If you want to support these devices in Win XP Sp2, add these patchs:
http://support.microsoft.com/kb/918365/
http://support.microsoft.com/kb/935892/
