[META version]
META version= ver 6.1232.0

[Main menu]
Menu selection =Update parameter
COM PORT =USB COM
Baseband chip =auto detect
Clock rate =
Flow control =software
Disable HW flow control = yes
GSM850 support =
Baudrate=Auto
Auto control power supply =yes
Boot timeout = infinite
META connect timeout = 120000
Power Supply On Off Count = 5
TST message format=
Authentication file=
Certificate file=
Com port filter=
Composite preloader= no
Preloader single port filter=VID_0E8D&PID_2000
Preloader composite port filter=VID_1004&PID_6000
BootROM com port filter=VID_0E8D&PID_0003
Kernel com port filter=

[Power supply table]
NORMAL_VOLTAGE = 3800
OFF_VOLTAGE = 0
CURRENT_LIMIT = 2000

[META factory]
DELAY_TIME_BEFORE_ACCESS_NVRAM = 10
Initial value from =ini file
RF calibration =yes
ADC calibration =no
TX PCL calibration =full pcl
RF calibration equipment=agilent 8960
Power Supply Type=agilent 661x
Barcode read from=file
Barcode save to=none
Auto start calibration enter=no
Barcode increasement enter=0
Read barcode from enter=none
Auto start calibration = yes
Turn off power supply when calibration fail =
Terminate META when calibration fail =no
Barcode increasement when calibration success=0
Terminate META when calibration success=
Turn off power supply when calibration success=
Terminate META when close =no
Save barcode to NVRAM when calibration success=no
Save barcode to file when calibration success=no
Barcode increasement when calibration fail=0
Save barcode to NVRAM when calibration fail=no
Save barcode to file when calibration fail=no
Terminate META exit=
Save barcode to NVRAM exit=no
Save barcode to file exit=no
Barcode increasement exit=0
663x2 GPIB Address =GPIB0::5::INSTR
661x GPIB Address =GPIB0::5::INSTR
Keithley 2306 GPIB Address = GPIB0::16::INSTR
E3631A GPIB Address = GPIB0::5::INSTR

AFC type=TCVCXO
AFC=yes
RX path loss=yes
TX PCL=yes
Crystal CAP ID=write NVRAM
PA type=RFMD3140
Sky77328 APC DC Offset cal = no
IP2=no
TX DC offset=no
TX AFC offset=no
Reset RF Tester=no
TX IQ calibration=no
WiFi TX DC offset calibration=no
WiFi TX power calibration=no
TX PCL type=2 pcl
BT crystal CAP ID calibration=no
GMSK TX PCL type=3 pcl
EPSK TX PCL type=full pcl
PA bias type=Fixed
TX PCL GMSK modulation=yes
TX PCL EPSK modulation=yes
WiFi calibration equipment=IQView
BT calibration equipment=CMU 200
WCDMA RSSI/LNA calibration=no
WCDMA TPC calibration=no
CV calibration=no
TX FB DAC calibraiton=no
TX slope skew calibration=no
Use BT equipment=no
FDT=no
WCDMA Temperature ADC=no
WiFi CAP ID calibration=no
WiFi Internal Sensor calibration=no
WCDMA AFC=no
WCDMA TPC Subband calibration=no
WCDMA TPC Power check=no
GMSK TX NSFT=no
BER NSFT=no
EPSK TX NSFT=no
WCDMA FHC=no
WCDMA NSFT TPC=no
WCDMA NSFT BER=no
WCDMA NSFT PRACH=no
Save barcode to NVRAM when calibration failed=no
Save barcode to file when calibration failed=no
Barcode increasement when calibration failed=0
Terminate META when calibration failed=
Turn off power supply when calibration failed=
Save barcode to NVRAM when calibration successfully=no
Save barcode to file when calibration successfully=no
Barcode increasement when calibration successfully=0
Terminate META when calibration successfully=
Turn off power supply when calibration successfully=
NVRAM database file=Y:\Tools\META\Test Case\Regression Loads\Apollo55v2\APOLLO55N_V2_DEMO_PCB01_tdd128hspa_MT6255_S00.MAUI_11B_W12_10.bin\BPLGUInfoCustomAppSrcP_MT6255_S00_MAUI_11B_W12_10
Configuration file=Z:\SharelibrarayVerify\Apollo55N_V2_TD\CFG_INI\MT6255_AST3001_20120615.cfg
Logging file=Z:\SharelibrarayVerify\Apollo55N_V2_TD\log.log
Result file=Z:\SharelibrarayVerify\Apollo55N_V2_TD\lg_result.txt
Calibration data initial file=Z:\SharelibrarayVerify\Apollo55N_V2_TD\CFG_INI\MT6255_AST3001_RF9811.ini
Calibration data result path=D:\mtk04126\Perforce\MTKWGT\tools\meta_app\customer_branches\v6.1236.0\MauiMETA_3G\Output
2G Calibration Item GGE Temperature ADC=no
2G Calibration Item AFC=yes
2G Calibration Item RX path loss=yes
2G Calibration Item W coefficient=no
2G Calibration Item TX FB DAC=no
2G Calibration Item TX PCL=yes
2G Calibration Item TX IQ=no
2G Calibration Item TX slope skew=no
2G Calibration Item TRX offset=no
2G NSFTGMSK TX=no
2G NSFTBER=no
2G NSFTEPSK TX=no
2G Calibration Item FHC=no
GMSK TX PCL2 PCL=no
GMSK TX PCL3 PCL=no
GMSK TX PCL6 DAC=no
GMSK TX PCLFull PCL=yes
GMSK TX PCLHigh Speed=no
EPSK TX PCL1 PCL=no
EPSK TX PCL2 PCL=no
EPSK TX PCL3 PCL=no
EPSK TX PCL4 PCL=no
EPSK TX PCLFull PCL=yes
EPSK TX PCLHigh Speed=no
TX PCL OptionGMSK=no
TX PCL OptionEPSK=no
TX PCL OptionDC offset Cal=no
TX PCL Option2G TX comp.=no
3G TDD Calibration Item3G TDD Temperature ADC=no
3G TDD Calibration Item3G TDD AFC=no
3G TDD Calibration Item3G TDD RX path loss=no
3G TDD Calibration Item3G TDD TPC=no
3G TDD NSFT3G TDD TX=no
3G TDD NSFT3G TDD BER=no
3G FDD Calibration Item3G FDD Temperature ADC=no
3G FDD Calibration Item3G FDD AFC=no
3G FDD Calibration Item3G FDD RX path loss=no
3G FDD Calibration Item3G FDD TPC=no
3G FDD TPCFDD Sub-band=no
3G FDD TPCPower check=no
3G FDD Calibration Item3G FDD FHC=no
3G FDD NSFT3G FDD TX=no
3G FDD NSFT3G FDD BER=no
3G FDD NSFTTX on/off Test=no
3G FDD NSFTHSDPA NSFT=no
3G FDD NSFTHSUPA NSFT=no
Other Calibration ItemADC=no
Other Calibration ItemBT Crystal CAP ID=no
Other Calibration ItemWiFi Crystal CAP ID=no
Other Calibration ItemWiFi Internal Sensor=no
Other Calibration ItemWiFi TX DC offset=no
Other Calibration ItemWiFi TX power=no
GMSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/712 PCL=no
GMSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/713 PCL=no
GMSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/716 DAC=no
GMSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/71Full PCL=yes
GMSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/71High Speed=no
EPSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/711 PCL=no
EPSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/712 PCL=no
EPSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/713 PCL=no
EPSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/714 PCL=no
EPSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/71Full PCL=yes
EPSK TX PCLRFMD 3140/46/66/96/98/4180/RF7161/66/70/71High Speed=no

[RF tool]
NVRAM database file=
TXPCS Configuration file=
TXPCS Logging file=

[8k Acoustic FIR Tunning]
Input file name=
Output TX file name=Output Rx file does not open
Output RX file name=Output Rx file does not open
Input ABS file name=
Direction=Rx
Boundary=3G Handset and Headset
Equipment=UPV
File Format=Linear
Field0_Hz=
Field0_Mag=
Field0_MagdB=
Field1_Hz=
Field1_Mag=                                                        
Field1_MagdB=
Field2_Hz=
Field2_Mag=
Field2_MagdB=
Field3_Hz=
Field3_Mag=
Field3_MagdB=
Field4_Hz=
Field4_Mag=
Field4_MagdB=
Field5_Hz=
Field5_Mag=
Field5_MagdB=
Field6_Hz=              
Field6_Mag=
Field6_MagdB=
Field7_Hz=
Field7_Mag=
Field7_MagdB=
Field8_Hz=
Field8_Mag=
Field8_MagdB=
Field9_Hz=
Field9_Mag=
Field9_MagdB=
Field10_Hz=
Field10_Mag=
Field10_MagdB=
Field11_Hz=
Field11_Mag=
Field11_MagdB=
Field12_Hz=
Field12_Mag=
Field12_MagdB=
Field13_Hz=
Field13_Mag=
Field13_MagdB=
Field14_Hz=
Field14_Mag=
Field14_MagdB=
                     
[16k Acoustic FIR Tunning]
Input file name=
Output TX file name=Output Tx file does not open
Output RX file name=Output Rx file does not open
Input ABS file name=
Boundary=3G Handset and Headset
Equipment=UPV
File Format=Linear
Field0_Hz=
Field0_Mag=
Field0_MagdB=
Field1_Hz=
Field1_Mag=
Field1_MagdB=
Field2_Hz=
Field2_Mag=
Field2_MagdB=
Field3_Hz=
Field3_Mag=
Field3_MagdB=
Field4_Hz=
Field4_Mag=
Field4_MagdB=
Field5_Hz=
Field5_Mag=
Field5_MagdB=
Field6_Hz=
Field6_Mag=
Field6_MagdB=
Field7_Hz=
Field7_Mag=
Field7_MagdB=
Field8_Hz=
Field8_Mag=
Field8_MagdB=
Field9_Hz=
Field9_Mag=
Field9_MagdB=
Field10_Hz=
Field10_Mag=
Field10_MagdB=
Field11_Hz=
Field11_Mag=
Field11_MagdB=
Field12_Hz=
Field12_Mag=
Field12_MagdB=
Field13_Hz=
Field13_Mag=
Field13_MagdB=
Field14_Hz=
Field14_Mag=
Field14_MagdB=
Field15_Hz=
Field15_Mag=
Field15_MagdB=
Field16_Hz=
Field16_Mag=
Field16_MagdB=

[32k Melody FIR Tunning]
Input file name=D:\Backup\Matlab\Louis\AudioTest\TRC1.TRC
Output TX file name=C:\Temp\test_Tx_FIR
Output RX file name=C:\Temp\test_Rx_FIR
Output file name=C:\Temp\par.ini

[IMEI Download]
IMEI = 12345678901234
NVRAM database file =

[MMI data download table]
download_type =associate 

[Default fullscreen file table]
DEFAULT_FULLSCREEN_PATH = c:\def_image\fullscreen\
MAX_FULLSCREEN_FILE_COUNT = 10
default_fullscreen_file_count=0

[Default assoicate file table]
DEFAULT_ASSOCIATE_PATH = c:\def_image\assoicate\
MAX_ASSOCIATE_FILE_COUNT = 10
default_assoicate_file_count=6

[Default EMS file table]
DEFAULT_EMS_PATH = c:\def_image\ems\
MAX_EMS_FILE_COUNT = 10
default_EMS_file_count=0

[Default midi file table]
DEFAULT_MIDI_PATH = c:\def_sound\other\
MAX_MIDI_FILE_COUNT = 10
default_midi_file_count=5
default_midi_file1=D:\Meta\Midi\Midi song\doraemon.mid
default_midi_file2=D:\Meta\Midi\Midi song\empire.mid
default_midi_file3=D:\Meta\Midi\Midi song\greenoil.mid
default_midi_file4=D:\Meta\Midi\Midi song\laputa.mid
default_midi_file5=D:\Meta\Midi\Midi song\mission.mid

[Default imelody file table]
DEFAULT_IMELODY_PATH = c:\def_sound\imelody\
MAX_IMELODY_FILE_COUNT = 10
default_imelody_file_count=1

[Audio Tool]
Play Song by FAT Filter Customized = .aac;.aif;.aiff;.amr;.au;.awb;.m4a;.mmf;.mp2;.wma;

[BT Tool]
HCI file=D:\Unzip\META\BT\HCI3.txt
MT6622 META NSR Support = no

[AEC]
NVRAM DB file=
Initial setting file=
audcoff_default_h=
Output speech FIR file=
Volume gain file=

[Audio Compensation FIR Tunning]
Freq DB mapping loudspeaker=0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.000
Freq DB mapping earphone=0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.000
Freq DB mapping loudspeaker ringtone=0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.00,0.000

[Dual-Mic. NR]
Sealing_THD=25
Step1Description=Record SLR pattern with the photo's configuration (main mic). The distance between mouth and main mic is 10cm. "With blocking" means covering glue  upon the mic hole.
Step2Description=Record SLR pattern with the photo's configuration (ref mic). The distance between mouth and ref mic is 10cm. "With blocking" means covering glue  upon the mic hole.
Step3Description=Record SLR pattern with the photo's configuration
Step4Description=Record SLR pattern with the photo's configuration. (normal position)
Step5Description=Record downlink wav, please make sure the receiver works well. (normal position)
Step6Description=Record SLR pattern with the photo's configuration. If the main mic hole is close to the left side, phone position is 20 degrees up, otherwise phone position is 20 degrees down.
Step7Description=Calculate coefficient based on the recorded file
