; Windows USB CDC ACM Setup File

; Based on INF template which was:
;     Copyright (c) 2000 Microsoft Corporation
;     Copyright (c) 2007 Microchip Technology Inc.
; likely to be covered by the MLPL as found at:
;    <http://msdn.microsoft.com/en-us/cc300389.aspx#MLPL>.
; For use only on Windows operating systems.

[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%MANU%
DriverVer=11/15/2007,5.1.2600.0

[Manufacturer]
%MANU%=DeviceList, NTamd64

[DestinationDirs]
DefaultDestDir=12


;------------------------------------------------------------------------------
;  Windows 2000/XP/Vista-32bit Sections
;------------------------------------------------------------------------------

[DriverInstall.nt]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.nt
AddReg=DriverInstall.nt.AddReg

[DriverCopyFiles.nt]
usbser.sys,,,0x20

[DriverInstall.nt.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,USBSER.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.nt.Services]
AddService=usbser, 0x00000002, DriverService.nt

[DriverService.nt]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\USBSER.sys

;------------------------------------------------------------------------------
;  Vista-64bit Sections
;------------------------------------------------------------------------------

[DriverInstall.NTamd64]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.NTamd64
AddReg=DriverInstall.NTamd64.AddReg

[DriverCopyFiles.NTamd64]
USBSER.sys,,,0x20

[DriverInstall.NTamd64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,USBSER.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NTamd64.Services]
AddService=usbser, 0x00000002, DriverService.NTamd64

[DriverService.NTamd64]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\USBSER.sys


;------------------------------------------------------------------------------
;  Vendor and Product ID Definitions
;------------------------------------------------------------------------------
; When developing your USB device, the VID and PID used in the PC side
; application program and the firmware on the microcontroller must match.
; Modify the below line to use your VID and PID.  Use the format as shown
; below.
; Note: One INF file can be used for multiple devices with different
;       VID and PIDs.  For each supported device, append
;       ",USB\VID_xxxx&PID_yyyy" to the end of the line.
;------------------------------------------------------------------------------
[SourceDisksFiles]

[SourceDisksNames]

[DeviceList]
%DESCRIPTION%=DriverInstall, USB\VID_0BB4&PID_0005&MI_02
%DESCRIPTION%=DriverInstall, USB\VID_0BB4&PID_0006
%DESCRIPTION%=DriverInstall, USB\VID_0525&PID_A4A7
%DESCRIPTION%=DriverInstall, USB\VID_0525&PID_A4A7&MI_00

; preloader VCOM
%VCOM%=DriverInstall, USB\Vid_0e8d&Pid_2000
%VCOM%=DriverInstall, USB\Vid_0e8d&Pid_0003

[DeviceList.NTamd64]
%DESCRIPTION%=DriverInstall, USB\VID_0BB4&PID_0005&MI_02
%DESCRIPTION%=DriverInstall, USB\VID_0BB4&PID_0006
%DESCRIPTION%=DriverInstall, USB\VID_0525&PID_A4A7
%DESCRIPTION%=DriverInstall, USB\VID_0525&PID_A4A7&MI_00

; preloader VCOM
%VCOM%=DriverInstall, USB\Vid_0e8d&Pid_2000
%VCOM%=DriverInstall, USB\Vid_0e8d&Pid_0003
;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------
;Modify these strings to customize your device
;------------------------------------------------------------------------------
[Strings]
MANU                = "MediaTek Inc."
DESCRIPTION         = "Gadget Serial"
SERVICE             = "USB RS-232 Emulation Driver"
VCOM                = "MediaTek USB VCOM (Android)"