From: <ÓÉ Microsoft Internet Explorer 5 ±£´æ>
Subject: Introduction
Date: Wed, 21 May 2008 17:13:48 +0800
MIME-Version: 1.0
Content-Type: multipart/related;
	type="text/html";
	boundary="----=_NextPart_000_0000_01C8BB66.08B88D70"
X-MimeOLE: Produced By Microsoft MimeOLE V6.00.2900.3028

This is a multi-part message in MIME format.

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: text/html;
	charset="Windows-1252"
Content-Transfer-Encoding: quoted-printable
Content-Location: file://D:\operate manual\V5.xx product tool\product tool 5 19en.htm

<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Transitional//EN">
<HTML><HEAD><TITLE>Introduction</TITLE>
<META http-equiv=3DContent-Type content=3D"text/html; =
charset=3Dwindows-1252">
<META content=3D"MSHTML 6.00.2900.3020" name=3DGENERATOR>
<STYLE>@font-face {
	font-family: SimSun;
}
@font-face {
	font-family: SimHei;
}
@font-face {
	font-family: SimSun;
}
@font-face {
	font-family: SimHei;
}
@page Section1 {size: 595.3pt 841.9pt; margin: 72.0pt 46.3pt 72.0pt =
54.0pt; layout-grid: 15.6pt; }
P.MsoNormal {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 10.5pt; MARGIN: 0cm 0cm 0pt; =
FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
LI.MsoNormal {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 10.5pt; MARGIN: 0cm 0cm 0pt; =
FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
DIV.MsoNormal {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 10.5pt; MARGIN: 0cm 0cm 0pt; =
FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
H1 {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 22pt; MARGIN: 17pt 0cm =
16.5pt; LINE-HEIGHT: 240%; FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: =
justify
}
H2 {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 16pt; MARGIN: 13pt 0cm; =
LINE-HEIGHT: 172%; FONT-FAMILY: Arial; TEXT-ALIGN: justify
}
H3 {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 16pt; MARGIN: 13pt 0cm; =
LINE-HEIGHT: 172%; FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
P.MsoCommentText {
	FONT-SIZE: 10.5pt; MARGIN: 0cm 0cm 0pt; FONT-FAMILY: "Times New Roman"
}
LI.MsoCommentText {
	FONT-SIZE: 10.5pt; MARGIN: 0cm 0cm 0pt; FONT-FAMILY: "Times New Roman"
}
DIV.MsoCommentText {
	FONT-SIZE: 10.5pt; MARGIN: 0cm 0cm 0pt; FONT-FAMILY: "Times New Roman"
}
P.MsoFooter {
	FONT-SIZE: 9pt; MARGIN: 0cm 0cm 0pt; LAYOUT-GRID-MODE: char; =
FONT-FAMILY: "Times New Roman"
}
LI.MsoFooter {
	FONT-SIZE: 9pt; MARGIN: 0cm 0cm 0pt; LAYOUT-GRID-MODE: char; =
FONT-FAMILY: "Times New Roman"
}
DIV.MsoFooter {
	FONT-SIZE: 9pt; MARGIN: 0cm 0cm 0pt; LAYOUT-GRID-MODE: char; =
FONT-FAMILY: "Times New Roman"
}
P.MsoDocumentMap {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 10.5pt; BACKGROUND: navy; =
MARGIN: 0cm 0cm 0pt; FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
LI.MsoDocumentMap {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 10.5pt; BACKGROUND: navy; =
MARGIN: 0cm 0cm 0pt; FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
DIV.MsoDocumentMap {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 10.5pt; BACKGROUND: navy; =
MARGIN: 0cm 0cm 0pt; FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
P.MsoCommentSubject {
	FONT-WEIGHT: bold; FONT-SIZE: 10.5pt; MARGIN: 0cm 0cm 0pt; FONT-FAMILY: =
"Times New Roman"
}
LI.MsoCommentSubject {
	FONT-WEIGHT: bold; FONT-SIZE: 10.5pt; MARGIN: 0cm 0cm 0pt; FONT-FAMILY: =
"Times New Roman"
}
DIV.MsoCommentSubject {
	FONT-WEIGHT: bold; FONT-SIZE: 10.5pt; MARGIN: 0cm 0cm 0pt; FONT-FAMILY: =
"Times New Roman"
}
P.MsoAcetate {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 9pt; MARGIN: 0cm 0cm 0pt; =
FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
LI.MsoAcetate {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 9pt; MARGIN: 0cm 0cm 0pt; =
FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
DIV.MsoAcetate {
	TEXT-JUSTIFY: inter-ideograph; FONT-SIZE: 9pt; MARGIN: 0cm 0cm 0pt; =
FONT-FAMILY: "Times New Roman"; TEXT-ALIGN: justify
}
SPAN.3Char {
	FONT-WEIGHT: bold; FONT-FAMILY: SimSun
}
DIV.Section1 {
	page: Section1
}
OL {
	MARGIN-BOTTOM: 0cm
}
UL {
	MARGIN-BOTTOM: 0cm
}
</STYLE>
</HEAD>
<BODY lang=3DZH-CN style=3D"TEXT-JUSTIFY-TRIM: punctuation">
<DIV class=3DSection1 style=3D"LAYOUT-GRID:  15.6pt none">
<H1><SPAN lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: =
240%">Introduction=20
</SPAN></H1>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Media Mass Product Tool is used =
to download=20
firmware to player from PC by USB transmission. The player shall have =
USB=20
communication function already. In order to improve manufacturing =
efficiency,=20
the solution is equipped with intelligent download tool to download =
firmware to=20
1~16 players via USB HUB simultaneously and give a completed download =
report.=20
With the help of the tool, manufacturer is able to have clear =
understanding on=20
daily manufacturing status by easily recording the information like the =
players=20
produced each day, quantity of error player. The tool is also able to=20
automatically copy test file, download hidden disk data and add virtual =
disk=20
image file to player (firmware support is required) while downloading =
firmware.=20
New functions are added to the tool of new version: self-help firmware =
download=20
after batch erase flash by U Disk, MTP device formatting. The following =
is an=20
example of mass production. </SPAN></P>
<H1><SPAN lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%">1 =
Installation=20
and uninstall</SPAN></H1>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">1.1=20
Software and hardware platform</SPAN></H2>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 21pt; LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">a. &nbsp;&nbsp;Tool =
installation package=20
</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 39pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: -18pt; =
LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US=20
style=3D"LINE-HEIGHT: =
150%">b.&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;Firmware</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 39pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: -18pt; =
LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US=20
style=3D"LINE-HEIGHT: =
150%">c.&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;Devcert=20
template. bin and private. bin. (Manufacturer has to purchase the =
license from=20
Microsoft.)</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 39pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: -18pt; =
LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: =
150%">d.&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; PC=20
with mainstream configuration, WINXP OS (self-prepared by=20
manufacturer)</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 44.2pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: =
-23.2pt; LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: =
150%">e.&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;USB=20
HUB, manufacturer could use &lt;=3D 16 Hubs, but the port number can't =
be over 16.=20
(USB 2.0, <SPAN style=3D"COLOR: black">OUTPUT: 5.0V---3.8Amax USB HUB is =

preferred, </SPAN>self-prepared by manufacturer).</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 39pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: -18pt; =
LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">f.&nbsp;&nbsp;&nbsp; USB =
cable</SPAN></P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">1.2=20
Install software</SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Open the installation package, =
double click=20
"Setup.exe" to enter setup interface, and click "next" to complete the=20
setup.</SPAN></P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">1.3=20
Uninstall software</SPAN></H2>
<P class=3DMsoNormal=20
style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: 150%; TEXT-ALIGN: left"=20
align=3Dleft><SPAN lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Two ways to =
uninstall the=20
tool: </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">a. =
Enter</SPAN><B><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">[</SPAN></B><SPAN =
lang=3DEN-US=20
style=3D"COLOR: black; LINE-HEIGHT: 150%">control panel</SPAN><B><SPAN =
lang=3DEN-US=20
style=3D"COLOR: black; LINE-HEIGHT: 150%">]</SPAN></B><SPAN lang=3DEN-US =

style=3D"COLOR: black; LINE-HEIGHT: 150%">-<B>[</B></SPAN><SPAN =
lang=3DEN-US=20
style=3D"COLOR: black; LINE-HEIGHT: 150%">add or delete =
program</SPAN><B><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">]</SPAN></B><SPAN =
lang=3DEN-US=20
style=3D"COLOR: black; LINE-HEIGHT: 150%">, select </SPAN><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">=93<SPAN style=3D"COLOR: black">Media</SPAN> =
Product=20
Tool=94, click "Delete" to uninstall it. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">b. Select=20
<B>[</B>start]-[program<B>]</B>, select </SPAN><SPAN lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">=93<SPAN style=3D"COLOR: black">Media</SPAN> =
Product=20
Tools:, click "Delete" to uninstall it </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%"></SPAN>&nbsp;</P>
<H1><SPAN lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%">2.=20
Settings</SPAN></H1>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">2.1=20
Run the Tool and identify USB port</SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Click<B> <SPAN=20
style=3D"COLOR: black">[s</SPAN></B><SPAN style=3D"COLOR: =
black">tart<B>]</B> <B>=96=20
[</B>program<B>]</B> and select =93Media Player</SPAN> Product Tool" - " =
<SPAN=20
style=3D"COLOR: black">Media Player</SPAN> Mass Product Tool ". If it is =
the first=20
time to use the tool, the system will first prompt =93whether to =
generate USB port=20
list=94 (select =93yes=94, the tool begin detecting USB port device; =
select =93no=94,=20
click =93identify port=94 button on the tool=92s main &nbsp;interface;) =
then =93import=20
firmware=94 window and =93import DRM file=94 windows will pop up =
(firmware support=20
required for DRM). The following main interface will show after correct =
firmware=20
and DRM file are added. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"><IMG height=3D478=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image001.jpg"=20
width=3D660></SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">In order to easily identify =
each USB port=20
of HUB, it is necessary to mark them before mass production. The =
procedure is as=20
follows: </SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 18pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: -18pt; =
LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">1.<SPAN=20
style=3D"FONT: 7pt 'Times New =
Roman'">&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;=20
</SPAN></SPAN><SPAN lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Click =
=93identify USB=20
port=94; </SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 18pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: -18pt; =
LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">2.<SPAN=20
style=3D"FONT: 7pt 'Times New =
Roman'">&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;=20
</SPAN></SPAN><SPAN lang=3DEN-US style=3D"LINE-HEIGHT: 150%">The tool =
could only=20
identify one USB port each time, so please connect to only one player at =
one=20
time (U Disk or ADFU device);</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 18pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: -18pt; =
LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">3.<SPAN=20
style=3D"FONT: 7pt 'Times New =
Roman'">&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;=20
</SPAN></SPAN><SPAN lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Identify =
USB port for=20
one time one by one. </SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 18pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: -18pt; =
LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">4.<SPAN=20
style=3D"FONT: 7pt 'Times New =
Roman'">&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;=20
</SPAN></SPAN><SPAN lang=3DEN-US style=3D"LINE-HEIGHT: 150%">The tool =
displays each=20
USB port number on the main interface one by one according to the order; =

</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 18pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: -18pt; =
LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">5.<SPAN=20
style=3D"FONT: 7pt 'Times New =
Roman'">&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;=20
</SPAN></SPAN><SPAN lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Identify =
each port of=20
HUB with tag at the same time and make it corresponding with the port =
number=20
displayed by the tool. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"><IMG height=3D478=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image002.jpg"=20
width=3D660></SPAN></P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">2.2=20
Import firmware </SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">Before =
downloading firmware,=20
make sure that the firmware version is correct, if new version is =
needed, click=20
=93import firmware=94 to choose the correct firmware to replace. Please =
see the=20
following screenshot: </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"FONT-SIZE: 9pt; COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D281=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image003.jpg"=20
width=3D480></SPAN></P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">2.3=20
Import DRM file (DRM support is required) </SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">If current =
firmware supports=20
DRM, the tool will notify that DRM file is required after importing =
firmware.=20
Click =93import DRM file=94, a dialogue window will pop up to require =
selecting=20
devcert template. bin and private. bin files, click =93OK=94 to finish. =
</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"FONT-SIZE: 9pt; COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D198=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image004.jpg"=20
width=3D312></SPAN></P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">2.4=20
Auto run File (firmware support is required)</SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">U disk auto run file =
realization is the=20
same as that of U Disk virtual driver auto run. Via making CDROM image, =
it can=20
burn image file and firmware into player to realize the function of auto =
run=20
file. It supports vista, winxp, win2k etc. </SPAN></P>
<P class=3DMsoNormal><SPAN class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; FONT-FAMILY: 'Times New =
Roman'">2.4.1</SPAN></SPAN><SPAN=20
lang=3DEN-US> Make auto run configuration file autorun.inf, the format =
is as=20
follows (for reference only):</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">[Autorun]</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">open=3Dsetup.exe</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">icon=3DCDRom.ico</SPAN></P>
<P class=3DMsoNormal><SPAN class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; FONT-FAMILY: 'Times New =
Roman'">2.4.2</SPAN></SPAN><SPAN=20
lang=3DEN-US> Save autorun.inf and CDRom.ico in the target file=92s dir. =
Target file=20
refers to the file which is going to be made as CDROM image.</SPAN></P>
<P class=3DMsoNormal><SPAN class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; FONT-FAMILY: 'Times New =
Roman'">2.4.3</SPAN></SPAN><SPAN=20
lang=3DEN-US> In main interface, select =93auto run=94 to enter CDROM =
image interface=20
and select the dir to make image. Click =93make=94 button to start and =
click =93OK=94=20
after it finishes. Click =93cancel=94 to cancel the operation. =
</SPAN></P>
<P class=3DMsoNormal><SPAN lang=3DEN-US></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D312=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image005.jpg"=20
width=3D516></SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal><SPAN class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; FONT-FAMILY: 'Times New =
Roman'">2.4.4</SPAN></SPAN><SPAN=20
lang=3DEN-US> If aut file already exists, directly select CDIMAGE image =
file add=20
aut, and click =93OK=94.</SPAN></P>
<P class=3DMsoNormal><SPAN lang=3DEN-US></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D314=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image006.jpg"=20
width=3D516></SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal><SPAN class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; FONT-FAMILY: 'Times New =
Roman'">2.4.5</SPAN></SPAN><SPAN=20
lang=3DEN-US> In the main interface, select (&#8730;) =93auto run=94. =
</SPAN></P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">2.5=20
Hidden Disk File (firmware support required) </SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">Hidden disk is to =
protect=20
file by hidden disk after player=92s mass product succeeds. In the main =
interface,=20
select =93hidden disk=94 </SPAN></P>
<P class=3DMsoNormal><SPAN class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; FONT-FAMILY: 'Times New =
Roman'">2.5.1</SPAN></SPAN><SPAN=20
lang=3DEN-US> User input</SPAN></P>
<P class=3DMsoNormal><SPAN lang=3DEN-US>No need to input =93volume=94 =
and =93start=20
address=94, use the default value. </SPAN></P>
<P class=3DMsoNormal><SPAN lang=3DEN-US>=93Actual size=94: size of the =
selected hidden=20
file, no need to input. </SPAN></P>
<P class=3DMsoNormal><SPAN lang=3DEN-US>=93Image from this directory=94: =
dir of the file=20
to be copied; can include sub dir. </SPAN></P>
<P class=3DMsoNormal><SPAN class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; FONT-FAMILY: 'Times New =
Roman'">2.5.2</SPAN></SPAN><SPAN=20
lang=3DEN-US> Hidden area type: </SPAN><SPAN lang=3DEN-US>FAT32 &amp; =
FAT16=20
optional.</SPAN></P>
<P class=3DMsoNormal><SPAN class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; FONT-FAMILY: 'Times New =
Roman'">2.5.3</SPAN></SPAN><SPAN=20
lang=3DEN-US> Click =93make=94 to make image, after it succeeds, click =
=93quit=94 to=20
finish. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D330=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image007.jpg"=20
width=3D648></SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><B><SPAN=20
lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN></B>&nbsp;</P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">2.6=20
Auto File copy (firmware support is required) </SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Auto copy is to copy the =
necessary file=20
into player when downloading firmware. It supports copying only with =
ADFU device=20
for now. </SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 17.7pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: =
-17.7pt; LINE-HEIGHT: 150%"><SPAN=20
class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 150%; FONT-FAMILY: 'Times New =
Roman'">2.6.1</SPAN></SPAN><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"> Connect to an ADFU device to =
let the tool=20
to read device=92s Flash capacity. The tool will pops up the device when =
reading=20
FLASH capacity. Re-plug USB cable after U disk image making finishes.=20
</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 5.9pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: =
-5.9pt; LINE-HEIGHT: 150%"><SPAN=20
class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 150%; FONT-FAMILY: 'Times New =
Roman'">2.6.2</SPAN></SPAN><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"> In the main interface, select =
=93support=20
auto copy=94 to enter U disk image maker (cancel the function by not =
selecting the=20
option). The tool will auto detect device=92s actual capacity. If disk =
image is=20
already made, select =93support auto copy=94, the system will notify =
=93disk image=20
exists already, whether to re-make=94, select =93yes=94 to re-make or =
select =93no=94 to=20
continue the original image. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 150%; FONT-FAMILY: 'Times New =
Roman'">2.6.3</SPAN></SPAN><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"> User input </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">=93Volume=94: U disk=92s =
volume, input according=20
to actual condition or no need to input.</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">=93Start address</SPAN><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%; FONT-FAMILY: Arial">=94</SPAN><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">:</SPAN><SPAN lang=3DEN-US =
style=3D"LINE-HEIGHT: 150%">=20
use the default value, no need to input. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">&nbsp;=93Actual size=94: =
normally, the tool=20
will read ADFU device=92s flash size and no need to input. Of course, =
users can=20
fill it if they are aware of the actual size (please refer to Note if =
auto read=20
of flash size fails) =93image from this directory=94 dir of the file to =
be copied;=20
can include sub dir. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 150%; FONT-FAMILY: 'Times New =
Roman'">2.6.4</SPAN></SPAN><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"> USB disk format</SPAN><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">: </SPAN><SPAN lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">FAT32 </SPAN><SPAN lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">&amp; </SPAN><SPAN lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">FAT16 optional</SPAN><SPAN lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">.</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
class=3D3Char><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 150%; FONT-FAMILY: 'Times New =
Roman'">2.6.5</SPAN></SPAN><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%"> Click =93make=94 to make =
image, after it=20
succeeds, click =93quit=94 to finish.</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D323=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image008.jpg"=20
width=3D648></SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 5.15pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: =
-5.15pt; LINE-HEIGHT: 150%"><B><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Notes: </SPAN></B><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">if the tool does not detect ADFU device or =
reading=20
FLASH capacity fails, user has to input FLASH capacity manually. Input =
FLASH=20
capacity like</SPAN><SPAN lang=3DEN-US style=3D"LINE-HEIGHT: 150%"> =
</SPAN><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">512</SPAN><SPAN lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">, </SPAN><SPAN lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">1024MB etc, the tool will auto calculate the =
actual U=20
disk capacity. </SPAN><SPAN lang=3DEN-US style=3D"LINE-HEIGHT: =
150%">Calculation=20
method:</SPAN><SPAN lang=3DEN-US> actual U disk capacity=3DFlash=20
capacity*0.95-firmware size, 0.05% of Flash capacity is used for Flash =
bad space=20
and size estimation value. Error may occur in this calculation, if error =
is too=20
obvious, it is necessary to adjust Flash capacity input. If the =
generated image=20
disk space increases, then increase Flash capacity or vice versa till =
the proper=20
capacity, see the following screenshot: </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D219=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image009.jpg"=20
width=3D360></SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D219=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image010.jpg"=20
width=3D360></SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US>2.6.6</SPAN><SPAN lang=3DEN-US> Re-make U disk image if =
mass production=20
player=92s FLASH capacity changes. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">2.7=20
Settings</SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">In main interface, click =
=93settings=94 to=20
enter configuration interface to set auto run parameters, the parameter =
is as=20
follows: </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Disable</SPAN><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">: do not auto detect auto run.</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">1,2,=85,16</SPAN><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">: After detecting&nbsp;the same number of =
devices=20
(include ADFU device and U disk), the tool starts mass production, the =
function=20
is the same as pressing =93start download=94 button.</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Mass production</SPAN><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">: the defaults is parallel, recommend =
choosing=20
parallel mass production to increase speed if using HUB to product =
multiply=20
players. If the player is directly connecting to PC=92s USB port instead =
of HUB,=20
sequence mode is required. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><B><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D437=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image011.jpg"=20
width=3D420></SPAN></B></P>
<H1><SPAN lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%">3. =
Mass=20
production </SPAN></H1>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">So the preparation for mass =
production=20
finishes. Next, connect the player to be upgraded to HUB port, the tool =
will=20
detect device one by one and display the current device number. The post =
number=20
will changes from grey to light blue. In addition, the tool report bar =
will=20
display four groups of data: total connected, total passed, current =
connected=20
and current passed. If current connected &lt; actual connected or =
current passed=20
&lt; current connected, then it indicates that player connection is not =
normal=20
or mass production fails. It can be tell from background color of port =
number:=20
grey, light blue, green and red, which represent device not connected, =
waiting=20
for mass production, mass production succeeds and mass production fails=20
respectively. &nbsp;</SPAN></P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">3.1=20
Start download</SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Click =93start download=94 to =
begin mass=20
production. Each download may continue for a couple of minutes. =
</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 0.1pt; LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D478=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image012.jpg"=20
width=3D660></SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 0.1pt; LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><B><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN></B>&nbsp;</P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">3.2=20
Finish mass production </SPAN></H2>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 0.1pt; LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">When mass =
production=20
finishes, the tool=92s main interface will show current passed number. =
Background=20
color of port number: successful (green), failed (red), please refer to =
the=20
following screenshot:</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 0.1pt; LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D478=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image013.jpg"=20
width=3D660></SPAN></P>
<H1><SPAN lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: =
240%">4</SPAN><SPAN=20
style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%; FONT-FAMILY: =
SimSun">&#65294;</SPAN><SPAN=20
lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%">MTP formatting =

</SPAN></H1>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">In XP OS, the tool supports =
simultaneous=20
MTP device formatting on multiply players. Click =93settings=94 on the =
main=20
interface, select =93MTP format=94, and connect to MTP device to be =
formatted.=20
Please use USB HUB when formatting multiply players. Then click =93start =
download=94=20
to format. The tool will show the connected and passed =
number.</SPAN></P>
<H1><SPAN lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: =
240%">5</SPAN><SPAN=20
style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%; FONT-FAMILY: =
SimSun">&#65294;</SPAN><SPAN=20
lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%"> Read =
LOG</SPAN></H1>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">Mass production =
completion=20
status: date, time, current connected number, total connected number, =
current=20
passed number, total passed number. Click =93read LOG=94 button to =
check. See the=20
following figure: </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"FONT-SIZE: 9pt; COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D350=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image014.jpg"=20
width=3D487></SPAN></P>
<H1><SPAN lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: =
240%">6</SPAN><SPAN=20
style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%; FONT-FAMILY: =
SimSun">&#65294;</SPAN><SPAN=20
lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%">Erase flash =
&amp; batch=20
upgrade</SPAN></H1>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">The functions of batch erase =
flash and auto=20
download firmware after erasing are added to the tool. It can batch =
upgrade 1~16=20
players of U disk status or of firmware upgrading status at the same =
time. The=20
operation is the same as that of the above-mentioned mass production. If =
the=20
firmware which is capable of erasing flash is desired, the firmware =
shall have=20
two functions: one is able to switch to U disk to ADFU status; the other =
is to=20
erase flash</SPAN><SPAN lang=3DEN-US style=3D"LINE-HEIGHT: =
150%">.</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">6.1=20
Select erased file</SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Select =93erase flash=94 in the =
main interface=20
to enter the interface as follows: </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D291=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image015.jpg"=20
width=3D480></SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Add the =93Firmware to enter =
ADFU mode=94 and=20
=93firmware to erase flash FW=94 files correctly. The firmware shall be =
the same.=20
Click =93OK=94 to continue or click =93cancel=94 to cancel the =
operation. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"><IMG=20
height=3D281=20
src=3D"file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%=
205%2019en.files/image016.jpg"=20
width=3D480></SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"COLOR: blue; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">6.2=20
Replace new firmware</SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">After erase file added and =
returning to the=20
main interface, click =93import firmware=94 to enter. The new firmware =
refers to the=20
correct firmware which is going to be downloaded to player. Please refer =
to=20
Section 2.2 for operation methods. </SPAN></P>
<H2><SPAN lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; LINE-HEIGHT: 172%; FONT-FAMILY: 'Times New =
Roman'">6.3=20
Start download</SPAN></H2>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">After the above operation =
finishes, click=20
</SPAN><SPAN lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%; FONT-FAMILY: Arial">=93</SPAN><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">start download</SPAN><SPAN lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%; FONT-FAMILY: Arial">=94</SPAN><SPAN =
lang=3DEN-US=20
style=3D"LINE-HEIGHT: 150%">, the tool will first the firmware for =
entering ADFU=20
to make player switches from U disk mode to ADFU mode; then download =
erase flash=20
firmware; finally download the correct new firmware. During the process, =
the=20
system will notify to install driver for ADFU device and the others will =
be=20
taken care by the tool automatically. If user wants to auto copy, auto =
run file=20
and make hidden disk while downloading firmware, please refer to Section =
2 to=20
configure the tool first then start download. =
&nbsp;&nbsp;&nbsp;</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><B><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">Notes for batch upgrade: =
</SPAN></B></P>
<P class=3DMsoNormal style=3D"MARGIN-LEFT: 18pt; TEXT-INDENT: =
-18pt"><SPAN=20
lang=3DEN-US>a.<SPAN=20
style=3D"FONT: 7pt 'Times New =
Roman'">&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;=20
</SPAN></SPAN><SPAN lang=3DEN-US>Before batch upgrade, make sure player =
to be=20
upgraded is formatted already and has only one partition.</SPAN></P>
<P class=3DMsoNormal style=3D"MARGIN-LEFT: 18pt; TEXT-INDENT: =
-18pt"><SPAN=20
lang=3DEN-US>b.<SPAN=20
style=3D"FONT: 7pt 'Times New =
Roman'">&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;=20
</SPAN></SPAN><SPAN lang=3DEN-US>In the process of batch upgrade, cannot =
do any=20
operation to U disk if player is under U disk status, otherwise the =
upgrade will=20
fail and the player cannot work normally. .</SPAN></P>
<P class=3DMsoNormal style=3D"MARGIN-LEFT: 18pt; TEXT-INDENT: =
-18pt"><SPAN=20
lang=3DEN-US>c.<SPAN=20
style=3D"FONT: 7pt 'Times New =
Roman'">&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;=20
</SPAN></SPAN><SPAN lang=3DEN-US>In WIN98/ME/2000, it cannot identify =
multiply=20
ADFU devices at the same time.</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><B><SPAN=20
lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN></B>&nbsp;</P>
<H1><SPAN lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: 240%">7. =
Delete=20
register trash file</SPAN></H1>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">After finishing =
firmware=20
download, insert USB cable to enter media device mode, PC registration =
will=20
generate VID&amp;PID file information. In order to guarantee PC=92s =
normal=20
working, please delete these information file periodically (please check =

player=92s VID&amp;PID before delete), the method is as =
follows:</SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">Click =
<B>[</B>start<B>]</B>=20
<B>-- [</B>run<B>]</B> and, input =93regedit=94 to run registration =
complier, select=20
&nbsp;HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlset\Enum\USB\vid_10d6&amp;p=
id_1101,=20
click right key to select =93permissions=94, &nbsp;select =93allow=94 in =
=93full control=94,=20
click the =93OK =93button, then vid_10d6&amp;pid_1101 dir is deleted =
</SPAN></P>
<H1><SPAN lang=3DEN-US style=3D"FONT-SIZE: 14pt; LINE-HEIGHT: =
240%">Notes for mass=20
production </SPAN></H1>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 15.4pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: =
-15.4pt; LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">a. Do not run =
other program=20
when running the tool in order to avoid interference.</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 15.4pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: =
-15.4pt; LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">b. The tool is =
able to=20
real-time check whether there is device connected, and the total =
connected=20
number and passed number will increase too, so no need to switch on and =
off=20
frequently. The total connection number will begin with 0 when the tool =
switches=20
on again. </SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 15.75pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: =
-15.75pt; LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">c.<SPAN style=3D"COLOR: black"> =
The HUB that=20
connecting to players usually will not make PC shutoff or re-start. If =
PC=20
shutoffs or restarts, it indicates that some player connecting to HUB =
has=20
serious error such as short circuit etc.</SPAN></SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 15.4pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: =
-15.4pt; LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"COLOR: black; LINE-HEIGHT: 150%">d. If several USB =
HUBs are=20
used at the same time, an USB extension cable is recommended for each=20
HUB.</SPAN></P>
<P class=3DMsoNormal=20
style=3D"MARGIN-LEFT: 15.4pt; LAYOUT-GRID-MODE: char; TEXT-INDENT: =
-15.4pt; LINE-HEIGHT: 150%"><SPAN=20
lang=3DEN-US style=3D"LINE-HEIGHT: 150%">e. PC will prompt =93find new =
hardware=20
wizard=94 when connecting USB port of PC or HUB to player at the first =
time,=20
manual driver installation are required. </SPAN></P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; COLOR: black; LINE-HEIGHT: 150%; FONT-FAMILY: =
Arial"></SPAN>&nbsp;</P>
<P class=3DMsoNormal style=3D"LAYOUT-GRID-MODE: char; LINE-HEIGHT: =
150%"><SPAN=20
lang=3DEN-US=20
style=3D"FONT-SIZE: 12pt; COLOR: black; LINE-HEIGHT: =
150%">[End]</SPAN></P></DIV></BODY></HTML>

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image001.jpg

[encoded data, 55936 characters]
r/6E1FZOv6tJ4j1Rr5EWGMKI0RuSAM9fzNFb85xtJu5//9k=

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image002.jpg

[encoded data, 57064 characters]

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image003.jpg

[encoded data, 29488 characters]
2Q==

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image004.jpg

[encoded data, 14436 characters]

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image005.jpg

[encoded data, 26296 characters]
pnduRg53Mc8Giip5myuWMdkbdFFFBZ//2Q==

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image006.jpg

[encoded data, 26512 characters]

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image007.jpg

[encoded data, 33432 characters]

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image008.jpg

[encoded data, 35492 characters]
DaQRMAcFIwCOPaiikFkfH0n+sb6miiigZ//Z

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image009.jpg

[encoded data, 12388 characters]
IHrsULn8qlopBYKKKKBn/9k=

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image010.jpg

[encoded data, 12312 characters]
uCIIY4geuxQufyqWikFgooooGf/Z

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image011.jpg

[encoded data, 23408 characters]
RgelFFABiloooAKKKKAP/9k=

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image012.jpg

[encoded data, 52896 characters]

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image013.jpg

[encoded data, 59204 characters]
2Q==

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image014.jpg

[encoded data, 50768 characters]
LgUUZhScJQh1UUvzHh7OLb7s/9k=

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image015.jpg

[encoded data, 22116 characters]
D//Z

------=_NextPart_000_0000_01C8BB66.08B88D70
Content-Type: image/jpeg
Content-Transfer-Encoding: base64
Content-Location: file:///D:/operate%20manual/V5.xx%20product%20tool/product%20tool%205%2019en.files/image016.jpg

[encoded data, 27132 characters]
xtd5+d1JLFSASAT64/Gu8o7UVnKTk9TWEVFWR//Z

------=_NextPart_000_0000_01C8BB66.08B88D70--
