; Installation inf for the Novatek 987 Boot Device
;
; (c) Copyright 2005 by Novatek
; All Right Reserved  
;
; Version 07/11/2005,1.0.0
;

[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
Provider="Novatek"        
Driverver=09/25/2009,1.0.1.05

[SourceDisksNames]
1="NVTK987 Installation Disk",,,

[SourceDisksFiles]
NVTK987.sys = 1
NVTK987.inf = 1

[Manufacturer]
%MfgName%=Microsoft

[Microsoft]
%USB\VID_0603&PID_8610.DeviceDesc%=NVTK987.Dev, USB\VID_0603&PID_8610


;[PreCopySection]
;HKR,,NoSetupUI,,1

[DestinationDirs]
NVTK987.Files.Ext = 10,System32\Drivers
NVTK987.Files.Inf = 10,INF

[NVTK987.Dev]
CopyFiles=NVTK987.Files.Ext, NVTK987.Files.Inf
AddReg=NVTK987.AddReg

[NVTK987.Dev.NT]
CopyFiles=NVTK987.Files.Ext, NVTK987.Files.Inf
AddReg=NVTK987.AddReg

[NVTK987.Dev.NT.Services]
Addservice = NVTK987, 0x00000002, NVTK987.AddService

[NVTK987.AddService]
DisplayName    = %NVTK987.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\NVTK987.sys
LoadOrderGroup = Base

[NVTK987.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,NVTK987.sys
HKLM,"System\Currentcontrolset\Services\NVTK987\Parameters","MaximumTransferSize",0x10001,4096
HKLM,"System\Currentcontrolset\Services\NVTK987\Parameters","DebugLevel",0x10001,1
HKLM,"System\Currentcontrolset\Services\NVTK987\Parameters","TrapEnable",0x10001,0

[NVTK987.Files.Ext]
NVTK987.sys

[NVTK987.Files.Inf]
NVTK987.Inf


;---------------------------------------------------------------;

[Strings]
Novatek="NOVATEK MICROELECTRONICS CORP."
MfgName="NOVATEK MICROELECTRONICS CORP."
USB\VID_0603&PID_8610.DeviceDesc="Novatek 98700 USB Firmware Update Device"
NOVATEK987.SvcDesc="NVTK987.Sys 987 Firmware Update driver, Version 1.0.0 "

